|  | **Tool** | **Name** | **Used for** |
| --- | --- | --- | --- |
| 1 | http://www-3.woodworktools.co.uk/faithfull-mini-combination-gauge-mtgco-00079240S.jpg | Mortice Gauge | Marking out mortice and tenon joints |
| 2 | http://www-4.woodworktools.co.uk/draper-64440-carpenters-marking-gauge-00067694S.jpg | Marking Gauge | Gauging parallel lines in wood |
| 3 | http://www-2.woodworktools.co.uk/emir-carpenters-mallet-00070057M.jpg | Wooden mallet | Striking chisels i.e. when chopping mortices |
| 4 | http://www-4.woodworktools.co.uk/faithfull-mini-try-square-mtts-00079234P.jpg | Try Square | Marking lines at 90 degrees, checking for squareness, usually in wood |
| 5 | **http://www-2.woodworktools.co.uk/draper-34049-100mm-precision-square-00064947M.jpg** | Engineer’s square | Marking lines at 90 degrees usually in metal and plastics |
| 6 | **http://www-2.woodworktools.co.uk/faithfull-carpenters-mitre-square-10in-00074403P.jpg** | Mitre Square | Marking lines at 45 degrees i.e. mitres |
| 7 | **http://www-4.woodworktools.co.uk/bahco-hgps06360-standard-axe-114lb-00072200M.jpg** | Axe (chopper) | Splitting wood (with the grain) |
| 8 | **http://www-3.woodworktools.co.uk/silverline-sl35-framing-square-600mm--00060926P.jpg** | Framing Square, roofing square | Marking out when cutting roof members or just checking for squareness |
| 9 | http://www-3.woodworktools.co.uk/silverline-633515-spoke-shave-convexed-00069605S.jpg | Spoke Shave  Can be curved or flat | For shaving wood when producing inside (concave) or outside (convex) curves |
| 10 | http://www-4.woodworktools.co.uk/silverline-wood-chisel-00069614S.jpg | Bevelled Edge Chisel | General purpose chisel for paring wood and removing waste |
| 11 | http://www-4.woodworktools.co.uk/faithfull-tools-faiwcarv3-straight-00093431M.jpg | Gouge | Making curved surfaces in wood |
| 12 | http://www-2.woodworktools.co.uk/faithfull-f0426-dome-head-chasing-00072340L.jpg | Bolster Chisel or Cold Chisel | Cutting bricks or concrete |
| 13 | http://www-2.woodworktools.co.uk/irwin-record-rec1366-1366-54in-t-bar-00096465S.jpg | Sash Clamp | Holding wood while glue dries |
| 14 | http://www-2.woodworktools.co.uk/faithfull-hobbyists-clamp-00069920M.jpg | G-Clamp | General purpose holding device |
| 15 | http://www-2.woodworktools.co.uk/black-decker-x52411-hinge-cutter-26mm-00078558M.jpg | Forstener drill bit | Producing flat bottomed holes in wood or drilling large holes in plastic |
| 16 | http://www-4.woodworktools.co.uk/silverline-633483-auger-bit-sds-5pce-00085979M.jpg | Wood Auger | Drilling holes in wood |
| 17 | http://www-4.woodworktools.co.uk/stanley-file-set-3pc-flat-12rnd-3-square-00102486M.jpg | Files | Shaping and finishing metal or plastics |
| 18 | http://www-2.woodworktools.co.uk/img/group/L/woodrasps.jpg | Surform | Shaping wood |
| 19 | http://www-1.woodworktools.co.uk/img/group/M/calipers.jpg | Dividers | Marking out cycles or curves on plastics and metal |
| 20 | http://www-4.woodworktools.co.uk/img/group/M/verniercalipers.jpg | Vernier Calliper | Accurate measurement – usually 0 – 150mm |
| 21 | http://www-2.woodworktools.co.uk/silverline-196600-depth-gauge-00100202S.jpg | Depth Gauge | Measuring the depth of holes |
| 22 | http://www-1.woodworktools.co.uk/faithfull-depth-gauge-with-protractor-00078909M.jpg | Protractor Depth Gauge | Measuring depth and angles |
| 23 | http://www-3.woodworktools.co.uk/silverline-245127-firm-joint-jenny-00100214M.jpg | Odd Leg Callipers | Marking out parallel lines |
| 24 | http://www-1.woodworktools.co.uk/faithfull-inside-spring-caliper-00083090S.jpg | Inside Callipers | Measuring inside measurements usually diameters of holes |
| 25 | http://www-3.woodworktools.co.uk/faithfull-outside-spring-caliper-00083091M.jpg | Outside Callipers | Measuring outside measurements often diameters of round objects |
| 26 | http://www-2.woodworktools.co.uk/silverline-196521-metric-dial-indicator-00100230S.jpg | Dial gauge indicator | Accurate measurement, part when using machines |
| 27 | http://www-2.woodworktools.co.uk/img/group/M/slidingbevels.jpg | Sliding Bevel | Measuring and marking angles |
| 28 | http://www-3.woodworktools.co.uk/img/group/M/stb96260g.jpg | Spirit Level | Checking for horizontal or vertical |
| 29 | http://www-4.woodworktools.co.uk/img/group/M/sta033719g.jpg | Tape Measure | Measuring and marking out usually above 300 mm |
| 30 | http://www-4.woodworktools.co.uk/dewalt-dew030p-dw030p-laser-distance-00090961S.jpg | Laser or Ultra Sound Measuring Device | Automatic measurement, still expensive but a thing of the future |
| 31 | http://www-2.woodworktools.co.uk/anti-vibe-claw-hammer-16oz-26119-00089977S.jpg | Claw Hammer | General carpentry use – knocking in nails and the claw for pulling them out |
| 32 | http://www-1.woodworktools.co.uk/silverline-hickory-shaft-ball-pein-00061233S.jpg | Ball Pein Hammer | General engineering work – the ball is often used for riveting |
| 33 | http://www-1.woodworktools.co.uk/draper-64595-joiners-or-warrington-00067711S.jpg | Cross Pei Hammer or Warrington Hammer | General purpose hammer – the cross pein is used for starting off small nails |
| 34 | http://www-3.woodworktools.co.uk/img/group/M/anvils.jpg | Anvil | General purpose support when working or beating metals |
| 35 | http://www-2.woodworktools.co.uk/faithfull-square-head-nail-punch-00069894S.jpg | Dot Punch, Centre Punch or Nail Punch | Dot – marking out  Centre – before drilling  Nail – punching in nails below the surface |
| 36 | http://www-2.woodworktools.co.uk/roughneck-dended-nail-puller-11in-00102609S.jpg | Crowbar or Wrecking Bar | Pulling out nails or breaking things apart |
| 37 | http://www-4.woodworktools.co.uk/draper-09246-draper-diy-series-250mm-00088798S.jpg | Tenon Saw | General purpose fine sawing of wood or sometimes plastic. Particularly Tenon joints. |
| 38 | http://www-1.woodworktools.co.uk/draper-general-purpose-hardpoint-handsaw-00062502S.jpg | Panel Saw, Rip Saw or Crosscut Saw | General purpose sawing of wood and large sheets of manufactured board |
| 39 | http://www-2.woodworktools.co.uk/draper-64408-coping-saw-frame-blade-00067691S.jpg | Coping Saw | Fine sawing of wood and plastics particularly for curved shapes |
| 40 | http://www-1.woodworktools.co.uk/draper-08704-draper-diy-series-junior-00088759S.jpg | Junior Hacksaw | Sawing of small items of plastics and metals |
| 41 | http://www-3.woodworktools.co.uk/tyson-pro-tools-300mm-12-hacksaw-00705013S.jpg | Hacksaw | General purpose saw for plastics and metals |
| 42 | http://www-4.woodworktools.co.uk/sealey-ak6093-smoothing-plane-00108204S.jpg | Smoothing Plane | Planing wood to get a smooth finish |
| 43 | http://www-2.woodworktools.co.uk/irwin-record-07-jointer-plane-238in-00074315M.jpg | Trying Plane or Jointing Plane | Making wood straight for joining. Where particular flatness or accuracy is required |
| 44 | http://www-2.woodworktools.co.uk/stanley-5-jack-plane-2in-112005-00074313S.jpg | Jack Plane | General purpose planing of wood |
| 45 | http://www-3.woodworktools.co.uk/img/group/M/rec778g.jpg | Rebate Plane | Planing rebates in wood. Planing right into the corner |
| 46 | http://www-3.woodworktools.co.uk/img/group/L/yankeescrewdrivers.jpg | Pump Screwdriver sometimes called a Yankee Screwdriver | Semi-automatic insertion or extraction of wood screws |
| 47 | http://www-1.woodworktools.co.uk/silverline-cb14-200mm-sharpening-stone-00069582S.jpg | Sharpening Stone, Oil Stone or Honing Stone | Final sharpening of woodworking tools particularly plane blades and chisels |
| 48 | http://www-1.woodworktools.co.uk/img/group/L/electricjigsaws110v.jpg | Jig Saw | General purpose sawing for wood, mainly for curves and when away from the bench |
| 49 | http://www-4.woodworktools.co.uk/dewalt-dewd23550-d23550-circular-saw-00091097S.jpg | Circular Saw | General purpose sawing of wood, mainly for straight cuts |
| 50 | http://www-2.woodworktools.co.uk/dewalt-dew738-dw738-bandsaw-two-speed-00091015S.jpg | Band Saw | General bench sawing of plastic and wood |
| 51 | http://www-3.woodworktools.co.uk/draper-48577-jointing-biscuits-no-0-pk-00066367M.jpg | Biscuits or Biscuit Joints | Joining wood together – reinforcing butt joints in wood |
| 52 | http://www-1.woodworktools.co.uk/silverstorm-128999-900w-biscuit-jointer-00084373S.jpg | Biscuit Jointer | Cutting slots for biscuit joints |
| 53 | http://www-1.woodworktools.co.uk/makita-3612-110v-12in-plunge-router-00117450S.jpg | Router | General purpose shaping of wood. Making mouldings and beading. |
| 54 | http://www.google.co.uk/url?source=imglanding&ct=img&q=http://3.bp.blogspot.com/-z8g9LLQEGq4/ThYRhbvG_0I/AAAAAAAAET0/WMz26daYUMg/s1600/Flat-Head-Screwdriver.jpg&sa=X&ei=5fgbT-LLJcWX8QPhlOGXCw&ved=0CAwQ8wc4Gg&usg=AFQjCNEnQoDGL_opK4OV3MVsv6uD7ffv1Q | Flat Point Screwdriver | Inserting or extracting slotted head screws |
| 55 | http://t0.gstatic.com/images?q=tbn:ANd9GcQNOIdEqEipJaoT8tJr-l1m77UebJDsT8BCoRCsWF9ZMGGdiCSKug | Star Point Screw Driver  Phillips Head, Posidrive Head | Inserting or extracting screws with star type heads |
| 56 | http://t2.gstatic.com/images?q=tbn:ANd9GcTpVfYimp66ILOZ1bPu65RUA3SM_uE1YvWreqTEug9pq-1Xk4UNVg | Micrometer | Measuring accurately usually 0 – 25 mm |